; Installation inf for the Intel 82930 USB Bulk IO Test Board
;
; (c) Copyright 1999 Microsoft
;

[Version]
Signature="$CHICAGO$"

Class=USB
ClassGUID={36fc9e60-c465-11cf-8056-444553540000} 
provider=%MSFT%
DriverVer=08/05/1999,5.00.2064
;CatalogFile=bulkusb.cat

[SourceDisksNames]
1=%Disk_Description%
2=%Disk_Description%
3=%Disk_Description%
4=%Disk_Description%

[SourceDisksFiles]
BULKUSB.sys = 1,\NTx86,
[SourceDisksFiles.ntx86]
BULKUSB.sys = 2,\NTx86,
[SourceDisksFiles.ntia64]
BULKUSB.sys = 3,\ntia64,
[SourceDisksFiles.ntamd64]
BULKUSB.sys = 4,\amd64,

[Manufacturer]
%MfgName%=Microsoft, ntx86, ntia64, ntamd64

[Microsoft]
%USB\VID_0919.DeviceDesc%=BULKUSB.Dev,USB\VID_0919&PID_0100

[Microsoft.ntx86]
%USB\VID_0919.DeviceDesc%=BULKUSB.Dev,USB\VID_0919&PID_0100

[Microsoft.ntia64]
%USB\VID_0919.DeviceDesc%=BULKUSB_ia64.Dev,USB\VID_0919&PID_0100

[Microsoft.ntamd64]
%USB\VID_0919.DeviceDesc%=BULKUSB_amd64.Dev,USB\VID_0919&PID_0100

[DestinationDirs]
BULKUSB.Files.Ext = 12
BULKUSB_ia64.Files.Ext = 12
BULKUSB_amd64.Files.Ext = 12
DefaultDestDir = 12  ; DIRID_DRIVERS 
                     ; == \System32\Drivers on Windows NT platforms
                     ; == \System\IoSubsys on Win9x platforms


[BULKUSB.Dev] 
CopyFiles=BULKUSB.Files.Ext
AddReg = BULKUSB.AddReg 
KnownFiles= BULKUSB.KnownFiles

[BULKUSB.Dev.nt]
CopyFiles=BULKUSB.Files.Ext
AddReg = BULKUSB.AddReg 
KnownFiles= BULKUSB.KnownFiles

[BULKUSB_ia64.Dev.nt]
CopyFiles=BULKUSB_ia64.Files.Ext

[BULKUSB_amd64.Dev.nt]
CopyFiles=BULKUSB_amd64.Files.Ext

[BULKUSB.Dev.nt.Services]
Addservice = BULKUSB, 0x00000002, BULKUSB.AddService

[BULKUSB.AddService]
DisplayName    = %BULKUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\BULKUSB.sys
AddReg         = BULKUSB.AddReg
LoadOrderGroup = Base

[BULKUSB.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,BULKUSB.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,"Parameters","BulkUsbEnable",0x10001,1
HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01

[BULKUSB_ia64.Dev.nt.Services]
Addservice = BULKUSB, 0x00000002, BULKUSB_ia64.AddService

[BULKUSB_ia64.AddService]
DisplayName    = %BULKUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\BULKUSB.sys
AddReg         = BULKUSB.AddReg
LoadOrderGroup = Base

[BULKUSB_ia64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,BULKUSB.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,"Parameters","BulkUsbEnable",0x10001,1
HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01

[BULKUSB_amd64.Dev.nt.Services]
Addservice = BULKUSB, 0x00000002, BULKUSB_amd64.AddService

[BULKUSB_amd64.AddService]
DisplayName    = %BULKUSB.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\BULKUSB.sys
AddReg         = BULKUSB.AddReg
LoadOrderGroup = Base

[BULKUSB_amd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,BULKUSB.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKR,"Parameters","BulkUsbEnable",0x10001,1

[BULKUSB.Files.Ext]
BULKUSB.sys

[BULKUSB_ia64.Files.Ext]
BULKUSB.sys

[BULKUSB_amd64.Files.Ext]
BULKUSB.sys

[BULKUSB.KnownFiles.x86]
BULKUSB.sys=safe

[BULKUSB_ia64.KnownFiles.x86]
BULKUSB.sys=safe

[BULKUSB_amd64.KnownFiles.x86]
BULKUSB.sys=safe

;---------------------------------------------------------------;

[Strings]
MSFT="Microsoft"
MfgName="Intel"
Disk_Description="BulkUsb Installation Disk"
USB\VID_0919.DeviceDesc="BulkUsb.Sys Sprinter Digital Level"
SprinterDesc="BulkUsb.Sys Sprinter digital level USB "
BULKUSB.SvcDesc="BulkUsb.Sys for Sprinter Digital Level"
LGT= "Leica Geosystems Technology" 
Desc_x860= "Spri